|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SCBA #** | **STEPS** | | | **Yes** | **No** |
| 1. All straps are fully extended and in good condition | | | |  |  |
| 1. Cylinder is a minimum 80% full | | | |  |  |
| 1. High Pressure hose connection is hand tight | | | |  |  |
| 1. Turn on cylinder – check for vibralert function in regulator | | | |  |  |
| 1. Check P.A.S.S. alarm function | | | |  |  |
| 1. Shoulder gauge and bottle gauge match (within 10% of each other is acceptable) | | | |  |  |
| 1. No leaks found in any hoses | | | |  |  |
| 1. Bleed down the system – vibralert functions at ¼ of shoulder gauge pressure | | | |  |  |
| Inspected By: | | Signature: | Date: | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **SCBA #** | **STEPS** | | | **Yes** | **No** |
| 1. All straps are fully extended and in good condition | | | |  |  |
| 1. Cylinder is a minimum 80% full | | | |  |  |
| 1. High Pressure hose connection is hand tight | | | |  |  |
| 1. Turn on cylinder – check for vibralert function in regulator | | | |  |  |
| 1. Check P.A.S.S. alarm function | | | |  |  |
| 1. Shoulder gauge and bottle gauge match (within 10% of each other is acceptable) | | | |  |  |
| 1. No leaks found in any hoses | | | |  |  |
| 1. Bleed down the system – vibralert functions at ¼ of shoulder gauge pressure | | | |  |  |
| Inspected By: | | Signature: | Date: | | |